Class A Honor Guard Uniform Guidelines

Coat: Fechheimer, 38800 Single Breasted, 11-11.5 oz. 100% VISA System 3 Polyester, Serge, LAPD Navy, Gold “S” Buttons, epaulets, metal badge tab, NO name tab.

· Officers and Sergeants shall have one double raised yellow/gold color #65 embroidered braid on each sleeve of the dress coat. The braid shall be ½ inch wide and positioned 3 inches from the edge of the cuff.

· Lieutenants shall have two double raised yellow/gold color #65 embroidered braids on each sleeve of the dress coat. Each braid shall be ½ inch wide and paced ¼ inch apart. The first braid shall be positioned 3 inches from the edge of the cuff.

· Captains shall have three double raised yellow/gold color #65 embroidered braids on each sleeve of the dress coat. Each braid shall be ½ inch wide and paced ¼ inch apart. The first braid shall be positioned 3 inches from the edge of the cuff.

· MNDOC shoulder patch both sleeves with Honor Guard rocker.

Pants: Fechheimer, 38200, 100% VISA System 3 Polyester Trousers, 11.5 -12 oz. SERGE weave, LAPD Navy, military slant hem. 
· Pants shall have one double raised yellow/gold color #65 braid on each pant leg. Each braid shall be 1 inch wide and placed centered on the outer seam.

Service Cap: Keystone, Round-Iowa Style Cap, A-5 Velcro Adjustable, Gold “S” Buttons. 

· Black chin band for Officers and Sergeants.

· Gold chin band for Lieutenants and Captains.  Premier Emblem & Insignia, P8004, Gold Metal Snake Style Cap Strap. 

· Proper wear position. The service cap is worn straight on the head so that the braid hatband on the service cap creates a straight line around the head, parallel to the ground. Such positioning automatically positions the visor correctly, so that it does not interfere with vision or ride up on the forehead. Personnel will not alter the shape of the service cap in any manner.

· Personnel will not wear headgear indoors unless under arms in an official capacity, or when directed, such as for indoor ceremonial activities.

Tie: Samuel Moore, 90001, polyester, navy, clip on.

Tie Bar: Hero’s Pride, X107902A, Minnesota Gold Tie Bar.

Socks: Socks shall be dark black.

Gloves: Deluxe Sure Grip, White, Velcro tab. 

Shoes: Bates, 942, Lites, High Gloss Oxford.

Shirt: Fechheimer, 35W7800, Long Sleeve, 100% VISA Polyester, Command.  
· MNDOC shoulder patch both sleeves with Honor Guard rocker.

Duty Belt: (3 Part)

· Jay-Pee, 402AC, 2 ¼ inch, Honor Guard Waist Belt with Gold Buckles, Clarino.

· Jay-Pee, 1435C, 1¼ inch, Shoulder Strap, Clarino

· Jay-Pee, S4428C, Slide on “D” Rings, Clarino.

Shoulder Cord: Premier Emblem & Insignia, P5509, French Single, Gold/Gold Tip. 

Name Plate:

· Coat: Green Tree, 250 Gold Matte, Gold Matte, Black Enamel, White Lettering. (Last name only).

· Shirt: Burlane, 238-DOC, MN DOC Name Tag (Gold/Black), Last name only.

· Both name plates are worn centered left to right on the flap of the right breast pocket, and centered between the top of the button and the top of the pocket.

Badge: Smith & Wesson, Gold Electroplate, Multi Color State Seal, Font – Block/Enamel – Black/Enamel Type - Regular, Curved.

· Coat: S93L, Shell Back, Clutch.

· Service Cap: S93, Screw.

Mourning Band: MinnCor, 1” Black Elastic Mourning Band.
· Black mourning bands shall be worn on the Honor Guard badge only in the following     circumstances;

· Wear a mourning band at the line of duty funeral of any corrections/law enforcement officer, or member of the United States armed forces, who died in the performance of duty.

· Wear a mourning band at the non-line of duty funeral of any active corrections/ law enforcement officer or retired corrections/law enforcement officer.

· Wear a mourning band on May 15th (National Peace Officers Memorial Day).

· At the discretion of your Honor Guard Team Leader, when special circumstances dictate the team display of mourning is appropriate.

· For the Honor Guard shield type badge, the mourning band should be horizontal on the badge and centered half way between the top and bottom.  The mourning band will only be worn on the shield type chest badge and not on the service cap badge.
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